STILMAT DICTATOR – Carpet - open
The DICTATOR  is the “strongest”  model among  all STILMAT aluminum doormats.  Specially reinforced aluminum construction (2 to 2.5 times comparing to the standard models),  where profiles are connected with thick  galvanized steel cable and rubber spacers.  This model fulfill the needs  of facilities with extreme visitors frequency and heavy duty roll-over and drive over capability of any kind of trolley and even forkliftsProfile standard clearance of 5 mm, or 3 mm available as an option for revolving door drives, in accordance with EN 16005. Imagine your impressive entrance with DICTATOR  STILMAT doormat. Suitable for internal use and for extreme frequency of passengers. This model is with high quality dust control carpet, ideal for picking up fine dirt and moisture  with 22mm height. The weather-proof solution among the robust solution. 

Flexible roll-up, extremely hard-wearing entrance mats produced to fit width and walking depth specifications perfectly. Suitable for wheeled traffic. Any geometric shape is available. STILMAT guarantee a custom spotless introduction to every entrance, because  it is a synonym  for aluminum doormats, modern and traditional glamour for every entrance and unique workman shift.

STILMAT DICTATOR – Carpet - open
Technical data
	Model
	 DICTATOR  (Carpet)

	Tread surface (inlay):
	High quality  dust control carpet, durable and  luxurious character. Made from 100% Polyamide. Weather-proof 

	Ideal for:
	Fine dirt and moisture

	Colors:
	Black, Grey, Brown…

	Version 
	Open system

	Code
	DOC

	Approx. height (mm)
	22

	Entrance position
	Indoors

	Zones: I – II - III
	Zone: III

	Load
	 Extreme

	Automatic door systems
	Profile clearance of 3 mm available as an option for revolving door drives, in accordance with EN 16005 

	Footfall
	Daily footfall of  2000 and up

	Roll-over and drive-over capability:
	Wheelchairs, Prams, Hand and Light shopping trolleys…Forklifts 

	Support chassis
	Made from rigid aluminum with rubber sound insulation underlay 

	Aluminum  material thickness (mm)
	2.5

	Connection
	Galvanized steel cable and rubber spacers

	Standard profile clearance approx. (mm)
	5 mm (or 3mm for automatic/revolving doors) 

	Slip resistance
	R 11 slip resistance as per DIN 51130

	Max  width/profile length for each individual section (mm):
	6000

	Max depth/walking depth for individual units (mm):
	Any

	Mat divisions as per factory standards or customer specifications
	Recommended   maximum mat weight of 45 kg 

	Depth for individual units  (mm):
	Cca 22

	Stationary load kg/100cm²
	4000

	Weight (kg/m²)
	Cca  30

	Logo options:
	Logo engraving

	Contact
	STILMAT


Guarantee: 5 years on aluminum parts and construction

STILMAT DICTATOR – Carpet - open
Text for invitation to tender
	Description:
	Flexible and roll-up, aluminum entrance mat for laying on the floor. Custom  produced mats  to fit width and walking depth specifications perfectly. Suitable for wheeled traffic. Any geometric shape is available on demand.

	Model
	 DICTATOR  (Carpet)

	Tread surface (inlay):
	High quality  dust control carpet, durable and  luxurious character. Made from 100% Polyamide 

	Ideal for:
	Fine dirt and moisture

	Colors:
	Black, Grey, Brown…

	Version 
	Open system

	Code
	DOC

	Approx. height (mm)
	22 mm

	Entrance position
	Indoors

	Zones: I – II - III
	Zone: III

	Load
	Extreme

	Automatic door systems
	Profile clearance of 3 mm available as an option for revolving door drives, in accordance with EN 16005 

	Footfall
	Daily footfall of 2000 and up

	Roll-over and drive-over capability:
	Wheelchairs, Prams, Hand and Light shopping trolleys…Forklifts

	Support chassis
	Made from rigid anodized aluminum with rubber sound insulation underlay 

	Aluminum coating:
	Fully anodized, to increase resistance to corrosion and wear. More aesthetically pleasing finish and harder surface than pure aluminum.

	Aluminum  material thickness (mm)
	2.5

	Connection
	Galvanized steel cable and rubber spacers

	Standard profile clearance approx. (mm)
	5 mm  (or 3mm for automatic/revolving doors)

	Slip resistance
	R 11 slip resistance as per DIN 51130

	Logo options:
	Logo engraving

	Contact
	STILMAT


