STILMAT EMPIRE Lux Brush/Ribbed carpet - open
EMPIRE is an optimal, wider and modern aludoormat, with double inlay. Imagine your impressive entrance with Empire STILMAT doormat. Extra wide for all buildings, with high demands with regard to resilience and harmonious appearance. Suitable for internal use and for normal to heavy  frequency of passengers. This model is with  thorough  brushes  for extra cleaning effect and high quality ribbed carpet. Ideal for picking up coarse dirt, fine dirt and moisture.  Anodized  aluminum doormat model with 24 mm height .

The weather-proof solution among the robust solution. 

Flexible roll-up, extremely hard-wearing entrance mat for laying on the floor. Mats produced to fit width and walking depth specifications perfectly. Suitable for wheeled traffic. Any geometric shape is available. 

STILMAT guarantee a custom spotless introduction to every entrance, because  it is a synonym  for aluminum doormats, modern and traditional glamour for every entrance and unique workman shift.

STILMAT EMPIRE Lux Brush/Ribbed carpet - open
Technical data
	Model
	 Empire (Lux brush & Ribbed carpet)

	Tread surface (inlay):
	Lux brushes recessed, robust and High quality ribbed carpet for Public buildings (A+EFL), durable and  luxurious character. Made from 100% Polyamide with gel backing. Weather-proof

	Ideal for:
	Coarse dirt, fine dirt and moisture

	Colors:
	Black, Grey, Brown…

	Version 
	Open system

	Code
	TOBL

	Approx. height (mm)
	24

	Entrance position
	Covered outdoor areas, gateways, passages

	Zones: I – II - III
	Zone: II

	Load
	 Heavy

	Footfall
	Daily footfall up to 2000

	Roll-over and drive-over capability:
	Wheelchairs, Prams, Hand and Light shopping trolleys 

	Support chassis
	Made from rigid anodized aluminum with rubber sound insulation underlay 

	Aluminum coating:
	Fully anodized, to increase resistance to corrosion and wear. More aesthetically pleasing finish and harder surface than pure aluminum. 

	Aluminum  material thickness (mm)
	1.2

	Connection
	Strong and flexible PVC connection strip, the entire width

	Standard profile clearance approx. (mm)
	5 mm (optional 3mm for automatic/revolving doors)

	Slip resistance
	R 11 slip resistance as per DIN 51130

	Max  width/profile length for each individual section (mm):
	6000

	Max depth/walking depth for individual units (mm):
	Any

	Mat divisions as per factory standards or customer specifications
	Recommended   maximum mat weight of 45 kg 

	Depth for individual units  (mm):
	Cca 24

	Stationary load kg/100cm²
	2200

	Weight (kg/m²)
	Cca  17

	Logo options
	Logo engraving

	Contact
	STILMAT


Guarantee: 5 years on aluminum parts and construction

STILMAT EMPIRE Lux Brush/Ribbed carpet - open
Text for invitation to tender
	Description:
	Flexible and roll-up, aluminum entrance mat for laying on the floor. Custom  produced mats  to fit width and walking depth specifications perfectly. Suitable for wheeled traffic. Any geometric shape is available on demand.

	Model
	 EMPIRE  (Lux brush & Ribbed carpet)

	Tread surface (inlay):
	Lux brushes recessed, robust and High quality ribbed carpet for Public buildings (A+EFL), durable and  luxurious character. Made from 100% Polyamide with gel backing. Weather-proof

	Ideal for
	Coarse dirt, fine dirt and moisture

	Colors:
	Black, Grey, Brown…

	Version 
	Open system

	Code
	TOBL

	Approx. height (mm)
	24 mm

	Entrance position
	Covered outdoor areas, gateways, passages

	Zones: I – II - III
	Zone: II

	Load
	From Normal to  Heavy

	Footfall
	Daily footfall up to 2000

	Roll-over and drive-over capability:
	Wheelchairs, Prams, Hand and Light shopping trolleys 

	Support chassis
	Made from rigid anodized aluminum with rubber sound insulation underlay 

	Aluminum coating:
	Fully anodized, to increase resistance to corrosion and wear. More aesthetically pleasing finish and harder surface than pure aluminum.

	Aluminum  material thickness (mm)
	1.2

	Connection
	Strong and flexible PVC connection strip, the entire width

	Standard profile clearance approx. (mm)
	5 mm (optional 3mm for automatic/revolving doors)

	Slip resistance
	R 11 slip resistance as per DIN 51130

	Logo options
	Logo engraving

	Contact
	STILMAT


