STILMAT EXECUTIVE – Ribbed carpet - open
EXECUTIVE aludoormat from STILMAT  is a top value deal . Like its name says, successful executive doormat, “budget- friendly”, which meets the basic characteristics of similar Stilmat models. It is a modern design aluminum doormat, with 23 mm height. STANDARD space between profiles guarantee to collect  dirt. Ideal for medium pit depth for picking up finedirt and moisture, with high quality ribbed carpet. Suitable for internal use, for entrances with normal visitor frequency. Imagine your impressive entrance with EXECUTIVE  STILMAT doormat. Flexible and roll-up, entrance mats produced to fit width and walking depth specifications perfectly. Suitable for wheeled traffic. Any geometric shape is available on demand. STILMAT guarantee a custom spotless introduction to every entrance, because  it is a synonym  for aluminum doormats, modern and traditional glamour for every entrance and unique workman shift.

STILMAT EXECUTIVE – Ribbed carpet - open
Technical data
	Model
	 EXECUTIVE  (Ribbed carpet)

	Tread surface (inlay):
	Lux brushes recessed, robust and  High quality ribbed carpet for Public buildings (A+EFL) , durable and  luxurious character. Made from 100% Polyamide with gel backing. Weather-proof

	Colors:
	Black, Grey, Brown…

	Ideal for
	Fine dirt and moisture

	Version 
	Open system

	Code
	EOL

	Approx. height (mm)
	23

	Entrance position
	Indoors

	Zones: I – II – III
	III

	Load
	 Normal

	Footfall
	Daily footfall up to 1000

	Roll-over and drive-over capability:
	Wheelchairs, Prams, Hand and Light shopping trolleys 

	Support chassis
	Made from rigid aluminum with rubber sound insulation underlay

	Aluminum  material thickness (mm)
	1.0

	Connection
	Strong and flexible PVC connection strip, the entire width

	Standard profile clearance approx. (mm)
	4.5  mm

	Slip resistance
	R 11 slip resistance as per DIN 51130

	Max  width/profile length for each individual section (mm):
	6000

	Max depth/walking depth for individual units (mm):
	Any

	Mat divisions as per factory standards or customer specifications
	Recommended   maximum mat weight of 45 kg 

	Depth for individual units  (mm):
	Cca 23

	Stationary load kg/100cm²
	1500

	Weight (kg/m²)
	Cca  19

	Logo options
	Logo engraving

	Contact
	STILMAT


Guarantee: 5 years on aluminum parts and construction

STILMAT EXECUTIVE – Ribbed Carpet - open
Text for invitation to tender
	Description:
	Flexible and roll-up, aluminum entrance mat for laying on the floor. Custom  produced mats  to fit width and walking depth specifications perfectly. Suitable for wheeled traffic. Any geometric shape is available on demand.

	Model
	 EXECUTIVE  (Ribbed carpet)

	Ideal for
	Fine dirt and moisture

	Tread surface (inlay):
	Lux brushes recessed, robust and   High quality ribbed carpet for Public buildings (A+EFL) , durable and  luxurious character. Made from 100% Polyamide with gel backing. Weather-proof

	Colors:
	Black, Grey, Brown…

	Version 
	Open system

	Code
	EOL

	Approx. height (mm)
	23 mm

	Entrance position
	Indoors

	Zones: I II III
	III

	Load
	Normal 

	Footfall
	Daily footfall up to 1000

	Roll-over and drive-over capability:
	Wheelchairs, Prams, Hand and Light shopping trolleys 

	Support chassis
	Made from rigid  aluminum with rubber sound insulation underlay

	Aluminum  material thickness (mm)
	1.0

	Connection
	Strong and flexible PVC connection strip, the entire width

	Standard profile clearance approx. (mm)
	4.5 mm

	Slip resistance
	R 11 slip resistance as per DIN 51130

	Logo options
	Logo engraving

	Contact
	STILMAT


