STILMAT KING – Lux Brush/Ribbed carpet - open
The KING is one of the base models of aluminum doormats, where profiles are connected with galvanized steel cable and rubber spacers. It is an alternative way of connection. Different and strong look. Proven design, rigid profiles. Profile standard clearance of 5 mm, or 3 mm available as an option for revolving door drives, in accordance with EN 16005. Imagine your impressive entrance with KING  STILMAT doormat. Suitable for internal use and for extreme frequency of passengers. This model is with  thorough  brushes  for an extra cleaning effect and  high quality ribbed carpet. Ideal for picking up coarse dirt, fine dirt and moisture. Anodized  aluminum doormat model with  24mm height. 
The weather-proof solution among the robust solution. Flexible roll-up, extremely hard-wearing entrance mats produced to fit width and walking depth specifications perfectly. Suitable for wheeled traffic. Any geometric shape is available. STILMAT guarantee a custom spotless introduction to every entrance, because  it is a synonym  for aluminum doormats, modern and traditional glamour for every entrance and unique workman shift.
STILMAT KING – Lux Brush/Ribbed carpet - open
Technical data
	Model
	 KING  (Lux Brush & Ribbed carpet)

	Tread surface (inlay):
	Lux brushes recessed, robust  and  High quality ribbed carpet for Public buildings (A+EFL) , durable and  luxurious character. Made from 100% Polyamide with gel backing. Weather-proof

	Ideal for:
	Coarse dirt, fine dirt and moisture

	Colors:
	Black, Grey, Brown…

	Version 
	Open system

	Code
	NOBL

	Approx. height (mm)
	24

	Entrance position
	Covered outdoor areas, gateways, passages

	Zones: I – II - III
	Zone: II

	Load
	 Extreme

	Automatic door systems
	Profile clearance of 3 mm available as an option for revolving door drives, in accordance with EN 16005 

	Footfall
	Daily footfall of  2000 and up

	Roll-over and drive-over capability:
	Wheelchairs, Prams, Hand and Light shopping trolleys 

	Support chassis
	Made from rigid anodized aluminum with rubber sound insulation underlay 

	Aluminum coating:
	Fully anodized, to increase resistance to corrosion and wear. More aesthetically pleasing finish and harder surface than pure aluminum. 

	Aluminum  material thickness (mm)
	1.2

	Connection
	Galvanized steel cable and rubber spacers

	Standard profile clearance approx. (mm)
	5 mm (or 3mm for automatic/revolving doors) 

	Slip resistance
	R 11 slip resistance as per DIN 51130

	Max  width/profile length for each individual section (mm):
	6000

	Max depth/walking depth for individual units (mm):
	Any

	Mat divisions as per factory standards or customer specifications
	Recommended   maximum mat weight of 45 kg 

	Depth for individual units  (mm):
	Cca 24

	Stationary load kg/100cm²
	2200

	Weight (kg/m²)
	Cca  20

	Logo options
	Logo engraving

	Contact
	STILMAT


Guarantee: 5 years on aluminum parts and construction

STILMAT KING – Lux Brush/Ribbed carpet - open
Text for invitation to tender
	Description:
	Flexible and roll-up, aluminum entrance mat for laying on the floor. Custom  produced mats  to fit width and walking depth specifications perfectly. Suitable for wheeled traffic. Any geometric shape is available on demand.

	Model
	 KING  (Lux Brush & Ribbed carpet)

	Tread surface (inlay):
	Lux brushes recessed, robust  and  High quality ribbed carpet for Public buildings (A+EFL) , durable and  luxurious character. Made from 100% Polyamide with gel backing. Weather-proof

	Ideal for:
	Coarse dirt, fine dirt and moisture

	Colors:
	Black, Grey, Brown…

	Version 
	Open system

	Code
	NOBL

	Approx. height (mm)
	24 mm

	Entrance position
	Covered outdoor areas, gateways, passages

	Zones: I – II - III
	Zone: II

	Load
	Extreme

	Automatic door systems
	Profile clearance of 3 mm available as an option for revolving door drives, in accordance with EN 16005 

	Footfall
	Daily footfall of 2000 and up

	Roll-over and drive-over capability:
	Wheelchairs, Prams, Hand and Light shopping trolleys 

	Support chassis
	Made from rigid anodized aluminum with rubber sound insulation underlay 

	Aluminum coating:
	Fully anodized  to increase resistance to corrosion and wear. More aesthetically pleasing finish and harder surface than pure aluminum.

	Aluminum  material thickness (mm)
	1.2

	Connection
	Galvanized steel cable and rubber spacers

	Standard profile clearance approx. (mm)
	5 mm  (or 3mm for automatic/revolving doors)

	Slip resistance
	R 11 slip resistance as per DIN 51130

	Logo options
	Logo engraving

	Contact
	STILMAT


